----------/etc/config/uLinux.conf----------
[System]
Model = TS-439
Internal Model = TS-439
Server comment = american
Version = 3.1.2
Build Number = 1014T
Time Zone = America/Phoenix
Enable Daylight Saving Time = TRUE
Workgroup = DODOES
Code Page = 437
System Device = /dev/sdx
Test Mode = FALSE 
Auto Create Raid = raid0
Wan Access = TRUE
Lan Access = TRUE
Web Access Port = 8080
E2KEY Support = FALSE
Rsync Support = TRUE
Rsync Model = QNAP
FS Type = ext3
Auto PowerOn = FALSE
Quota Type = vfsv0
Write Connection Log = 0

Booting = 0
Server Name = american
UPNP_UUID = 76c5f8aa-558a-40f7-a07e-3f4ea6ab79ff
Redundant Power Enable = FALSE
[Test]
Test Program = /sbin/test/Self-test-main

[NTP]
USE NTP Server = FALSE
NTP Server IP = pool.ntp.org
Enable NTP Server = FALSE
Server1 IP =
Server2 IP =
Sercer3 IP =
Interval = 1
TimeUnit = DAY

[Alert]
Alert Level = 0
SMTP IP = 0.0.0.0
Alert Mail = 
SMS Mode = 0

[Network]
Interface Number = 2
DNS = 0.0.0.0
WINS IP = 0.0.0.0
WINS Enable = False
BONDING Support = TRUE
BONDING01 = Interface1
BONDING02 = Interface2
Domain Name Server 1 = 0.0.0.0
Domain Name Server 2 = 0.0.0.0
[bond0]
Bonding Mode = 4
Configure = TRUE
Use DHCP = TRUE
Usage = DHCP
IP Address = 169.254.100.100
Subnet Mask = 255.255.0.0
Broadcast = 169.254.255.255
Gateway = 169.254.100.100
Speed = auto
MTU = 1500

[eth0]
Configure = False
Use DHCP = TRUE
Usage = DHCP
IP Address = 169.254.100.100
Subnet Mask = 255.255.0.0
Broadcast = 192.168.255.255
Gateway = 169.254.100.100
Speed = auto
MTU = 1500

[eth1]
Configure = False
Use DHCP = TRUE
Usage = DHCP
IP Address = 169.254.100.100
Subnet Mask = 255.255.0.0
Broadcast = 192.168.255.255
Gateway = 169.254.100.100
Speed = auto
MTU = 1500

[Samba]
Enable = TRUE
[Appletalk]
Enable = TRUE
Default Zone = *
[SNMP]
Server Enable = FALSE

[WebFS]
Enable = TRUE
Web Root Path = /WWW

[QWEB]
Enable = 1
Port = 80
[QPHOTO]
Enable = TRUE
[BTDownload]
Enable = TRUE
Max_Running = 3
Qget_Support = TRUE
Download_Folder = /share/Qdownload/
Total Job = 0
Run List Job = 0
Pause List Job = 0
Finish List Job = 0
Overwrite List = 0
Max Download Rate = 0
Max Upload Rate = 0
Port Range From = 6881
Port Range To = 6999
UPnP Port Forwarding = 0
encrypt = 0
DT Time = 1
S1 Enable = 0
S2 Enable = 0
[NVR]
Enable = FALSE
Support = TRUE

[Storage]
Auto Init = FALSE
Disk Drive Number = 4
Drive 1 = sda
Drive 2 = sdb
Drive 3 = sdc
Drive 4 = sdd
Disk Check On Boot = Error
Auto Fix Disk Check Errors = TRUE
Support RAID 5 = FALSE
SUPPORT HOTSWAP = TRUE
Support Hot Spare = FALSE
Support LVM = FALSE

Encrypt_sda3 = FALSE
Encrypt_sdb3 = FALSE
Encrypt_sdc3 = FALSE
Encrypt_md0 = FALSE
[Disk]
Drive 1 EXIST = 1
Drive 2 EXIST = 1
Drive 3 EXIST = 1
Drive 4 EXIST = 0
Drive 5 EXIST = 0

Drive 13 EXIST = 0
Drive 9 EXIST = 1
[FTP]
ServerName = ProFTPD
Enable = False
Port = 21
MaxInstances = 30
User = guest
Group = guest
DefaultRoot = /share
MaxAnonymous = 30
AllowAnonymous = False
Unicode = 0
CharsetRemote = 999
SSL MODE = 1
Passive Enabled = 1
Bandwidth Enabled = 0
Max connection per account = 10
EnableUserWanIp = FALSE
WanIp = 
[DHCP Server]
Enable = FALSE
Start Range = 169.254.1.100
End Range = 169.254.1.200
Max Lease Time = 86400

[Printers]
Support = FALSE
Enable = False
Name =
Comment = Printer port on NAS

Phy exist = 0
Phy exist2 = 0
Phy exist3 = 0
Phy exist4 = 0
Phy exist5 = 0
[LOGO]
Show PIC Index = 1
PIC Counter = 10
Default LOGO Image Path = /etc/config/logo/default_logo_img.gif
Upload LOGO Image Path = /etc/config/logo/upload_logo_img.gif
PIC1 LOGO Image Path = /etc/config/logo/pic1_logo_img.gif
PIC2 LOGO Image Path = /etc/config/logo/pic2_logo_img.gif
PIC3 LOGO Image Path = /etc/config/logo/pic3_logo_img.gif
PIC4 LOGO Image Path = /etc/config/logo/pic4_logo_img.gif
PIC5 LOGO Image Path = /etc/config/logo/pic5_logo_img.gif
LOGO Image Size Limitation = 20480

[UPS]
Support = TRUE
Serial UPS = FALSE
Snmp UPS = TRUE
Daemon Type = 1
UPS IP = 0.0.0.0
Enable = FALSE
UPS Type = PhxTec-A1000
Shutdown System In = 5
ValidCOM = 1
AC Power = OK
Battery Power = OK

[Misc]
Disk StandBy Timeout = 5
Disk StandBy Timeout Enable = TRUE
Disk Free Size Alert = 3072
Disk Free Size Alert Enable = TRUE
Buzzer Warning Enable = TRUE
Wake On Lan = FALSE

System Started = TRUE
Configured = TRUE
Reset Password Switch = TRUE
Custom Temp = 0
system low temp = 40
system high temp = 48
[HWTEST]
mini PCI = Agere Systems

[MySQL]
Enable = FALSE
DB_Init = FALSE
[LOGIN]
SSH Enable = TRUE
SSH Port = 22
TELNET Enable = FALSE
TELNET Port = 13131

[Index]
Qphoto_LOGO = FALSE
Qdownlod_LOGO = FALSE

[iSCSI]
Company Info = 2004-04.com.qnap
Model Name = TS-439
[END_FLAG]
[usb copy]
usb_copy_avail = 1
lock flag = 0
usb copying = 0
copy func old = 0
copy func = 0
internal = Qusb
copy type = 0
[UPnP Service]
Enable = TRUE
[NFS]
Enable = TRUE
[TwonkyMedia]
Enable = TRUE
[iTune]
Enable = TRUE
Password Enabled = 0
Code Page = CP437
[Bonjour Service]
Web = 1
Web Service Name = american
SAMBA = 1
SAMBA Service Name = american(SAMBA)
AFP = 1
AFP Service Name = american(AFP)
SSH = 0
SSH Service Name = american(SSH)
FTP = 0
FTP Service Name = american(FTP)
[QRAID1]
device name = 
