smartctl version 5.38 [x86_64-redhat-linux-gnu] Copyright (C) 2002-8 Bruce Allen
Home page is http://smartmontools.sourceforge.net/

Device: SEAGATE ST3146855LW Version: 0003
Serial number: 3LN38VV300001234X9Y9
Device type: disk
Transport protocol: Parallel SCSI (SPI-4)
Local Time is: Wed Jan 6 11:12:33 2010 CET
Device supports SMART and is Enabled
Temperature Warning Enabled
SMART Health Status: FAILURE PREDICTION THRESHOLD EXCEEDED [asc=5d, ascq=0]

Current Drive Temperature:   41 C
Drive Trip Temperature:      68 C
Vendor (Seagate) cache information
 Blocks sent to initiator = 2530286685
 Blocks received from initiator = 69995041
 Blocks read from cache and sent to initiator = 369926188
 Number of read and write commands whose size <= segment size = 285052588
 Number of read and write commands whose size > segment size = 2
Vendor (Seagate/Hitachi) factory information
 number of hours powered up = 14396.07
 number of minutes until next internal SMART test = 49

Error counter log:
           Errors Corrected by           Total   Correction     Gigabytes    Total
               ECC          rereads/    errors   algorithm      processed    uncorrected
           fast | delayed   rewrites  corrected  invocations   [10^9 bytes]  errors
read:   31670228     7327         0  31677555   31677510       1071.313          63
write:         0        0         0         0          0   15728656813.914           0
verify:   527341        3         0    527344     527452        131.461           0

Non-medium error count: 1618

[GLTSD (Global Logging Target Save Disable) set. Enable Save with '-S on']

SMART Self-test log
Num  Test              Status                 segment  LifeTime  LBA_first_err [SK ASC ASQ]
     Description                              number   (hours)
# 1  Background long   Interrupted ('-X' switch)   -   14394                 - [-   -    -]

Long (extended) Self Test duration: 1367 seconds [22.8 minutes]
